****

**PopUp WiFi Express**

Compact powerful high availability WiFi unit with external ethernet port and battery compatibility. Suitable for high density situations and more remote areas.

**Quick Facts**

Runs using three 4G/LTE-Advanced cellular providers concurrently for increased performance and 99.9% uptime.

Ideal for video streaming.

CAPTIVATE compatible.

Crowd counting and presence-analytics compatible.

GPS Tracking available.

**Dimensions**

21.7 x 13.8 x 9 inches

23lb

**Router**

Multi-provider capable (AT&T, Verizon, T-Mobile)

200Mbps throughput

8 Load-balancing algorithms

Static public IP address capable

Cloud-managed

High-gain antennas for superior 4G performance

16 VLANs

**Access Point**

100 concurrent users

CAPTIVATE compatible

3x3 MIMO antenna

5GHz and 2.4GHz (5GHz recommended)

Complies with all major WiFi security standards

Web content filtering / application filtering

Cloud-managed

**Power**

Powered by standard US 3-pin AC power plug

Battery power available via external 4 pin XLR connector.

Low power consumption (approx. 30 watts)

Compatible with generators

**Build**

Tough hard case construction

Approved to take as carry on or checked in luggage.

Combination Locked – able to be opened by airport security (TSA approved)

Splash resistant.

4-pin xlr power (for battery power)

Green power indicator light

External Ethernet – CAT6A For connecting a network switch, direct client access or external WAN.