****

**PopUp WiFi Go HD**

Compact, powerful, high-availability WiFi unit with external ethernet port and battery compatibility.

**Quick Facts**

Runs two 4G/LTE-Advanced cellular providers concurrently.

CAPTIVATE compatible.

Crowd counting and presence analytics compatible.

GPS Tracking available.

Not for live video streaming.

**Dimensions**

12.2 x 10.6 x 7.8 in

11lb

**Router**

Multi-provider capable (AT&T, Verizon, T-Mobile)

100Mbps throughput

8 Load-balancing algorithms

Static public IP address capable

Cloud-managed

Medium-gain antennas for high 4G performance

16 VLANs

**Access Point**

25 concurrent users

CAPTIVATE compatible

2x2 MIMO

5GHz and 2.4GHz (5GHz recommended)

Complies with all main WiFi security standards

Web content filtering / application filtering

Cloud-managed

**Power**

Powered by standard US 3-pin AC power plug

Battery power available via external 4 pin XLR connector.

Low power consumption (approx. 20 watts)

Compatible with generators

**Build**

Rugged hard case construction.

Splash resistant.

Approved to take as carry-on or checked baggage on planes.

Locked, can be opened by airport security (TSA approved)

4 pin XLR power inlet to connect to battery power.

Green power indicator light.

External Ethernet – CAT6A for connecting a network switch, direct client access or external WAN.